<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.22.14-Bia?owie?a">
  <identifier>小班_確定版_相双</identifier>
  <parentidentifier></parentidentifier>
  <language>JPN</language>
  <type>dataset</type>
  <title>小班_確定版_相双</title>
  <abstract></abstract>
  <contact>
    <name></name>
    <organization></organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email></email>
    <role></role>
  </contact>
  <links/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys>
      <wkt>PROJCRS["JGD2000 / Japan Plane Rectangular CS IX",BASEGEOGCRS["JGD2000",DATUM["Japanese Geodetic Datum 2000",ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4612]],CONVERSION["Japan Plane Rectangular CS zone IX",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",36,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",139.833333333333,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.9999,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",0,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["northing (X)",north,ORDER[1],LENGTHUNIT["metre",1]],AXIS["easting (Y)",east,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Cadastre, engineering survey, topographic mapping (large and medium scale)."],AREA["Japan - onshore - Honshu - Tokyo-to. (Excludes offshore island areas of Tokyo-to covered by Japan Plane Rectangular Coordinate System zones XIV, XVIII and XIX)."],BBOX[29.31,138.4,37.98,141.11]],ID["EPSG",2451]]</wkt>
      <proj4>+proj=tmerc +lat_0=36 +lon_0=139.833333333333 +k=0.9999 +x_0=0 +y_0=0 +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>420</srsid>
      <srid>2451</srid>
      <authid>EPSG:2451</authid>
      <description>JGD2000 / Japan Plane Rectangular CS IX</description>
      <projectionacronym>tmerc</projectionacronym>
      <ellipsoidacronym>EPSG:7019</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial maxz="0" crs="EPSG:2451" maxx="0" minx="0" miny="0" minz="0" dimensions="2" maxy="0"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
